{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":62,"n_cols":3,"rows_kept":62,"cut":false,"hidden":false,"merged":[]}
["Modbus地址","参数","描述"]
["0x1000","脉冲发送端子","0-Y0口输出\r\n1-Y1口输出\r\n2-Y2口输出\r\n3-Y3口输出"]
["0x1001","脉冲方向端子","0-Y12口输出\r\n1-Y13口输出\r\n2-Y14口输出\r\n3-Y15口输出"]
["0x1002","EXT信号","0-X4口输入\r\n1-X5口输入"]
["0x1003","脉冲方向延时时间","单位：ms"]
["0x1004","脉冲方向逻辑","0-正逻辑\r\n1-负逻辑"]
["0x1005","脉冲加减速模式","0-直线加减速\r\n1-S曲线加减速\r\n2-正弦曲线加减速"]
["0x1006","运行模式","0-相对\r\n1-绝对"]
["0x1007","脉冲总段数（1~10）"]
["0x1008","起始执行段数"]
["0x1009~0x100A","脉冲默认速度","单位：HZ"]
["0x100B","脉冲默认速度加速时间","单位：ms"]
["0x100C","脉冲默认速度减速时间","单位：ms"]
[]
["0x1100~0x1101","第1段脉冲频率","单位：HZ"]
["0x1102~0x1103","第1段脉冲个数(可设置负数)"]
["0x1104","第1段等待条件","0-脉冲发送完成\r\n1-EXT信号"]
["0x1105","第1段跳转编号"]
["0x1110~0x1111","第2段脉冲频率","单位：HZ"]
["0x1112~0x1113","第2段脉冲个数(可设置负数)"]
["0x1114","第2段等待条件","0-脉冲发送完成\r\n1-EXT信号"]
["0x1115","第2段跳转编号"]
["0x1120~0x1121","第3段脉冲频率","单位：HZ"]
["0x1122~0x1123","第3段脉冲个数(可设置负数)"]
["0x1124","第3段等待条件","0-脉冲发送完成\r\n1-EXT信号"]
["0x1125","第3段跳转编号"]
["0x1130~0x1131","第4段脉冲频率","单位：HZ"]
["0x1132~0x1133","第4段脉冲个数(可设置负数)"]
["0x1134","第4段等待条件","0-脉冲发送完成\r\n1-EXT信号"]
["0x1135","第4段跳转编号"]
["0x1140~0x1141","第5段脉冲频率","单位：HZ"]
["0x1142~0x1143","第5段脉冲个数(可设置负数)"]
["0x1144","第5段等待条件","0-脉冲发送完成\r\n1-EXT信号"]
["0x1145","第5段跳转编号"]
["0x1150~0x1151","第6段脉冲频率","单位：HZ"]
["0x1152~0x1153","第6段脉冲个数(可设置负数)"]
["0x1154","第6段等待条件","0-脉冲发送完成\r\n1-EXT信号"]
["0x1155","第6段跳转编号"]
["0x1160~0x1161","第7段脉冲频率","单位：HZ"]
["0x1162~0x1163","第7段脉冲个数(可设置负数)"]
["0x1164","第7段等待条件","0-脉冲发送完成\r\n1-EXT信号"]
["0x1165","第7段跳转编号"]
["0x1170~0x1171","第8段脉冲频率","单位：HZ"]
["0x1172~0x1173","第8段脉冲个数(可设置负数)"]
["0x1174","第8段等待条件","0-脉冲发送完成\r\n1-EXT信号"]
["0x1175","第8段跳转编号"]
["0x1180~0x1181","第9段脉冲频率","单位：HZ"]
["0x1182~0x1183","第9段脉冲个数(可设置负数)"]
["0x1184","第9段等待条件","0-脉冲发送完成\r\n1-EXT信号"]
["0x1185","第9段跳转编号"]
["0x1190~0x1191","第10段脉冲频率","单位：HZ"]
["0x1192~0x1193","第10段脉冲个数(可设置负数)"]
["0x1194","第10段等待条件","0-脉冲发送完成\r\n1-EXT信号"]
["0x1195","第10段跳转编号"]
[]
[]
["0x2000~0x2001","脉冲个数监控值（可读取负数）"]
[]
[]
["0x3000","脉冲发送按钮","按下“发送脉冲”按钮后，向0x3000地址写1；\r\n抬起“发送脉冲”按钮后，向0x3000地址写2；"]
[]
["上位机使用说明：\r\n1，正确设置COM口、波特率\r\n2，点击“通信连接”，上位机会读取PLC参数值，并对界面值进行更新\r\n3，点击“写入参数”，将界面值写入PLC中\r\n4，点击“发送脉冲”，触发PLC进行脉冲输出"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}